



* Socket programing
* Token bucket r ekta pyq chherechhilam bubu& RBR token bucket 27, 28
* Virtual circuiting (6.swithcing)
* Wrap around vid 4, 5








In iisc dns authoritative server the database is maintained csa.iisc.in or ece.iisc.in webpage contain which ip address.












































For 2 routers it can work properly but fot for more it may fail.

